Gocator API > Go2 > Constants > GO2_DEFAULT_IP_MASK

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

GO2_DEFAULT_IP_MASK
Constants
Description

Default sensor IP mask ("255.255.255.0").

C

    #define GO2_DEFAULT_IP_MASK (0xFFFFFF00)            // Default sensor IP mask ("255.255.255.0").

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference