Gocator API > Go2 > Classes > Go2Sensor > Functions > Go2Sensor_SetActiveAreaWidth

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2Sensor_SetActiveAreaWidth
Functions
Description

Sets the active area width.

C

    Go2Status Go2Sensor_SetActiveAreaWidth(Go2Sensor sensor, Go2Double width);

Parameters

Parameters | Description
Go2Sensor sensor | Go2Sensor object.
Go2Double width | Active area width (mm).

Returns

Operation status.

File

Go2Sensor.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference