Gocator API

- Home
- Categories
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Groups Pages
Types
Classes, interfaces, structures, enumerations, and simple values:

C GoActiveAreaConfig | Represents an active area configuration element
C GoAddressInfo | Sensor network address settings
C GoAlignmentRef | Represents an alignment reference
C GoAlignmentState | Represents an alignment state
C GoAlignmentTarget | Represents a alignment target type
C GoAlignmentType | Represents an alignment type
C GoAlignMsg | Represents a message containing an alignment result
C GoAnalog | Represents Analog output settings
C GoAnalogEvent | Represents a analog output event
C GoAnalogTrigger | Represents an analog output trigger
C GoAsciiOperation | Represents an ASCII protocol operational type
C GoControl | Represents a set of sensor command connections (control, upgrade)
C GoDataMessageType | Lists all data message types
C GoDataMsg | Represents a base message sourced from the data channel
C GoDataSet | Represents a collection of data channel or health channel messages
C GoDataSource | Represents a data source
C GoDecision | Represents the measurement output decision values. Bit 0 represents the decision value, while bits 1 through 7 represent the decision code, outlined by GoDecisionCode
C GoDecisionCode | Represents the possible measurement decision codes
C GoDigital | Represents Digital output settings
C GoDigitalEvent | Represents a digital output event
C GoDigitalPass | Represents a digital output condition
C GoDigitalSignal | Represents a digital output signal type
C GoDiscovery | Represents a discovery client
C GoDiscoveryInfo | Represents discovery information for a single device
C GoElement32u | Represents a 32-bit unsigned integer configuration element with a range and enabled state
C GoElement64f | Represents a 64-bit floating point configuration element with a range and enabled state
C GoEncoderSpacingMinSource | Represents the current encoder period limiting source
C GoEncoderTriggerMode | Represents an encoder's triggering behavior
C GoEthernet | Represents Ethernet output settings
C GoEthernetProtocol | Represents a ethernet output protocol
C GoExposureCalMsg | Represents a message containing exposure calibration results
C GoExposureMode | Represents all possible exposure modes
C GoFamily | Represents the supported Gocator hardware families
C GoFrameRateMaxSource | Represents the current maximum frame rate limiting source
C GoHealthIndicatorId | Represents a health indicator ID
C GoHealthMsg | Represents health information from a single sensor
C GoIndicator | Represents health indicator
C GoInputSource | Represents a data input source
C GoLayout | Represents a layout related sensor configuration
C GoMeasurement | Represents the base class for a tool measurement or script output
C GoMeasurementData | Represents a measurement result
C GoMeasurementMsg | Represents a message containing a set of GoMeasurementData
C GoMeasurementType | Lists all measurement types
C GoMode | Represents a scan mode
C GoMultiplexBank | Represents a bank of related sensors to be used in multiplexing
C GoOrientation | Represents a sensor orientation type
C GoOutput | Represents output configuration
C GoOutputDelayDomain | Represents an output delay domain
C GoOutputSource | Represents output sources
C GoPixelType | Represents a video message pixel type
C GoRangeIntensityMsg | Represents a data message containing a set of range intensity data
C GoRangeMsg | Represents a data message containing a set of range data
C GoRangePosition | Represents a range position tool
C GoRangePositionZ | Represents a position Z measurement of a Range Position tool
C GoRangeThickness | Represents a range thickness tool
C GoRangeThicknessThickness | Represents a the thickness measurement of a Range Thickness tool
C GoRangeTool | Represents a base range tool
C GoReceiver | Represents a data/health receiver
C GoReplayExportSourceType | Represents the replay export source type
C GoRole | Represents a user role
C GoScript | Represents a script tool
C GoScriptOutput | Represents a script output for a Script Tool
C GoSeekDirection | Represents a playback seek direction
C GoSelcomFormat | Represents the selcom format followed on the serial output
C GoSensor | Represents a Gocator sensor
C GoSensorInfo | Represents read-only sensor information
C GoSerial | Represents Serial output settings
C GoSerializer | Serializes/deserializes objects to/from Gocator Data Protocol
C GoSerialProtocol | Represents all serial output protocols
C GoSetup | Represents a device configuration
C GoSpacingIntervalType | Represents spacing interval types
C GoStamp | Represents an acquisition stamp
C GoStampMsg | Represents a message containing a set of acquisition stamps
C GoState | Represents the current state of a sensor object
C GoStates | Sensor state, login, alignment information, recording state, playback source, uptime, playback information, and auto-start setting state
C GoSystem | Represents a system of Gocator devices
C GoTool | Represents the base tool class
C GoTools | Represents a collection of tools
C GoToolType | Lists all tool types
C GoTransform | Represents a sensor transformation
C GoTransformation | Represents an alignment element
C GoTransformedDataRegion | Represents a transformed data region
C GoTrigger | Represents a trigger
C GoTriggerSource | Represents a trigger source type
C GoTriggerUnits | Represents the system's primary synchronization domain
C GoUpgradeFxArgs | Represents arguments provided to an upgrade callback function
C GoUser | Represents a user id
C GoVideoMsg | Represents a data message containing a video image