Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSystem_UpdateAllMultiplexParameters | ( | GoSystem | system,
|  | k64f | period
| ) |  |

Automatically update the single multiplexing delay and period configuration for all sensors contained in all defined multiplex banks.

Version
  Introduced in firmware 4.0.10.27

Parameters

  system | GoSystem object.
  period | The exposure period to set among all multiplexed sensors. A value of 0.0 will result in automatic period determination.

Returns
  Operation status.