Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_ScheduleDigital | ( | GoControl | control,
|  | k16u | index,
|  | k64s | target,
|  | k8u | value
| ) |  |

Schedules a digital output.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  index | The digital output index.
  target | The time or position target (uS or mm), depending on the configured domain. Ignored if scheduling disabled or pulsed mode enabled.
  value | The value of scheduled output (0-Low or 1-High). Ignored if pulsed mode enabled.

Returns
  Operation status.