Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_BeginExposureAutoSet | ( | GoControl | control,
|  | GoRole | role
| ) |  |

Sends an exposure auto set command to a sensor, but doesn't wait for the response.

Use the GoControl_EndExposureAutoSet function to wait for the sensor's reply.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  role | The sensor's role.

Returns
  Operation status.

See also
  GoControl_EndExposureAutoSet