Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoReceiver_Open | ( | GoReceiver | receiver,
|  | kIpAddress | address,
|  | k32u | port
| ) |  |

Opens a data connection to the specified sensor IP address and port.

Version
  Introduced in firmware 4.0.10.27

Parameters

  receiver | Receiver object.
  address | Sensor IP address.
  port | Sensor data port.

Returns
  Operation status.