Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoLayout_SetOrientation | ( | GoLayout | layout,
|  | GoOrientation | orientation
| ) |  |

Sets the buddied sensor configuration orientation.

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.
  orientation | The orientation to set.

Returns
  Operation status.