Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoEthernet_SetAsciiOperation | ( | GoEthernet | ethernet,
|  | GoAsciiOperation | mode
| ) |  |

Sets the ASCII operation mode.

Version
  Introduced in firmware 4.0.10.27

Parameters

  ethernet | GoEthernet object.
  mode | The selected ASCII operation mode.

Returns
  Operation status.