Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoDigital_AddSource | ( | GoDigital | digital,
|  | k32u | sourceId
| ) |  |

Selects the specified decision source for use in determining pass/fail status.

Version
  Introduced in firmware 4.0.10.27

Parameters

  digital | GoDigital object.
  sourceId | Index of the source to be added/selected.

Returns
  Operation status.