Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_Reset | ( | GoSensor | sensor,
|  | kBool | wait
| ) |  |

Reboots the main sensor and any connected buddy sensors.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  wait | kTRUE to wait for reboot and then reconnect.

Returns
  Operation status.