Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoLayout_SetMultiplexSinglePeriod | ( | GoLayout | layout,
|  | k64f | value
| ) |  |

Sets the single sensor multiplexing period.

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.
  value | The multiplexing period (in uS) to set.

Returns
  Operation status.