Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoMultiplexBank_RemoveSensor | ( | GoMultiplexBank | bank,
|  | k32u | id
| ) |  |

Removes a sensor from the given multiplexing bank.

Version
  Introduced in firmware 4.0.10.27

Parameters

  bank | GoMultiplexBank object.
  id | The ID of the sensor in the bank to the remove.

Returns
  Operation status.