Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetSpacingInterval | ( | GoSetup | setup,
|  | GoRole | role,
|  | k64f | value
| ) |  |

Sets the spacing interval.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  value | The spacing interval.

Returns
  Operation status.