Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Member Functions
GoLayout Class Reference
GoSdk

## Description

Represents a layout related sensor configuration.

Inheritance diagram for GoLayout:

## Public Member Functions
GoOrientation | GoLayout_Orientation (GoLayout layout)
| Returns the current orientation used when buddied. More...
kStatus | GoLayout_SetOrientation (GoLayout layout, GoOrientation orientation)
| Sets the buddied sensor configuration orientation. More...
k64f | GoLayout_TransformedDataRegionHeight (GoLayout layout)
| Returns the transformed data region height value. More...
k64f | GoLayout_TransformedDataRegionLength (GoLayout layout)
| Returns the transformed data region length value. More...
k64f | GoLayout_TransformedDataRegionWidth (GoLayout layout)
| Returns the transformed data region width value. More...
k64f | GoLayout_TransformedDataRegionX (GoLayout layout)
| Returns the transformed data region X-component value. More...
k64f | GoLayout_TransformedDataRegionY (GoLayout layout)
| Returns the transformed data region Y-component value. More...
k64f | GoLayout_TransformedDataRegionZ (GoLayout layout)
| Returns the transformed data region Z-component value. More...
k64f | GoLayout_XSpacingCount (GoLayout layout)
| Returns the layout specific X spacing count value. More...
k64f | GoLayout_YSpacingCount (GoLayout layout)
| Returns the layout specific Y spacing count value. More...

The documentation for this class was generated from the following file:

- GoLayout.h