Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensorInfo_Model | ( | GoSensorInfo | info,
|  | kChar * | model,
|  | k32u | capacity
| ) |  |

Gets the model string of the sensor which provided the sensor information.

Version
  Introduced in firmware 4.0.10.27

Parameters

  info | GoSensorInfo object.
  model | A character array pointer.
  capacity | The character array capacity.

Returns
  Operation status.