Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Types
GoSdk

## Description

Core types and definitions.

## Types
struct | GoActiveAreaConfig
| Represents an active area configuration element. More...
struct | GoAddressInfo
| Sensor network address settings. More...
struct | GoAlignmentRef
| Represents an alignment reference. More...
struct | GoAlignmentState
| Represents an alignment state. More...
struct | GoAlignmentStatus
| Represents the operation status of an alignment. More...
struct | GoAlignmentTarget
| Represents a alignment target type. More...
struct | GoAlignmentType
| Represents an alignment type. More...
struct | GoDataSource
| Represents a data source. More...
struct | GoDecision
| Represents the measurement output decision values. Bit 0 represents the decision value, while bits 1 through 7 represent the decision code, outlined by GoDecisionCode. More...
struct | GoDecisionCode
| Represents the possible measurement decision codes. More...
struct | GoElement32u
| Represents a 32-bit unsigned integer configuration element with a range and enabled state. More...
struct | GoElement64f
| Represents a 64-bit floating point configuration element with a range and enabled state. More...
struct | GoElementBool
| Represents a boolean configuration element with an enabled state. More...
struct | GoEncoderSpacingMinSource
| Represents the current encoder period limiting source. More...
struct | GoEncoderTriggerMode
| Represents an encoder's triggering behavior. More...
struct | GoExposureMode
| Represents all possible exposure modes. More...
struct | GoFamily
| Represents the supported Gocator hardware families. More...
struct | GoFrameRateMaxSource
| Represents the current maximum frame rate limiting source. More...
struct | GoGammaType
| Represents a material gamma type. More...
struct | GoImageType
| Represents an image type. More...
struct | GoImplicitTriggerOverride
| Represents an EthernetIP implicit messaging trigger override. More...
struct | GoInputSource
| Represents a data input source. More...
class | GoLayout
| Represents a layout related sensor configuration. More...
class | GoMeasurement
| Represents the base class for a tool measurement or script output. More...
struct | GoMode
| Represents a scan mode. More...
struct | GoOrientation
| Represents a sensor orientation type. More...
struct | GoPartFrameOfReference
| Represents a part detection frame of reference. More...
struct | GoPatternSequenceType
| Represents a pattern sequence type. More...
struct | GoPixelType
| Represents a video message pixel type. More...
struct | GoReplayExportSourceType
| Represents the replay export source type. More...
struct | GoRole
| Represents a user role. More...
struct | GoSeekDirection
| Represents a playback seek direction. More...
class | GoSensor
| Represents a Gocator sensor. More...
class | GoSensorInfo
| Represents read-only sensor information. More...
class | GoSetup
| Represents a device configuration. More...
struct | GoSpacingIntervalType
| Represents spacing interval types. More...
struct | GoState
| Represents the current state of a sensor object. More...
struct | GoStates
| Sensor state, login, alignment information, recording state, playback source, uptime, playback information, and auto-start setting state. More...
class | GoSystem
| Represents a system of Gocator devices. More...
class | GoTransform
| Represents a sensor transformation. More...
struct | GoTransformation
| Represents an alignment element. More...
struct | GoTransformedDataRegion
| Represents a transformed data region. More...
struct | GoTrigger
| Represents a trigger. More...
struct | GoTriggerSource
| Represents a trigger source type. More...
struct | GoTriggerUnits
| Represents the system's primary synchronization domain. More...
struct | GoUpgradeFxArgs
| Represents arguments provided to an upgrade callback function. More...
struct | GoUser
| Represents a user id. More...