Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_EndExposureAutoSet | ( | GoControl | control | ) |

Waits for a exposure auto set response from a sensor.

Call this function sometime after calling BeginExposureAutoSet.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.

Returns
  Operation status.