Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoSetup_ActiveAreaHeightLimitMin | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the minimum valid value for the ActiveAreaHeight setting.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.

Returns
  Minimum valid ActiveAreaHeight value (mm).