Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoSetup_TransformedDataRegionZ | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the transformed data region Z value.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | The device whose value to retrieve.

Returns
  The transformed data region Z value.