| MikroCAD SDK Library

- Home
- All Types
- Files

All Classes Files Functions Variables Typedefs Enumerations Enumerator Macros Pages
MeasurementErrorCodes.h
Go to the documentation of this file.
1 /**
2 * @file MeasurementErrorCodes.h
3 * @brief MikroCAD SDK Error codes
4 *
5 * @author LMI Technologies
6 */
7
8 #ifndef _MeasurementErrorCodes_h
9 #define _MeasurementErrorCodes_h
10
11 /**
12 Error codes
13 */
14 enum MeasurementErrorCode
15 {
16 MeasurementErrorCode_None = 0, /**< No error */
17
18 // Common errors
19
20 MeasurementErrorCode_NotInitialized = -1, /**< Not or incorrect initialized */
21 MeasurementErrorCode_Initializing = -2, /**< Error on initializing */
22 MeasurementErrorCode_FunctionNotImplemented = -3, /**< Function is not implemented */
23 MeasurementErrorCode_InvalidVersion = -4, /**< Invalid version of a software component */
24 MeasurementErrorCode_InvalidFileFormat = -5, /**< Invalid file format */
25 MeasurementErrorCode_FileSaveError = -6, /**< Cannot save file */
26
27 MeasurementErrorCode_SensorLibrary = -11, /**< Error on loading sensor library */
28 MeasurementErrorCode_SensorLibraryFunc = -12, /**< Error on loading sensor library function */
29
30 MeasurementErrorCode_BufferLocked = -21, /**< A buffer is locked */
31 MeasurementErrorCode_CheckSumError = -22, /**< Check sum error */
32
33 MeasurementErrorCode_DirectoryNotExists = -31, /**< Directory not exists */
34 MeasurementErrorCode_FileNotExists = -32, /**< File not exists */
35 MeasurementErrorCode_FileAlreadyExists = -33, /**< File already exists */
36
37 MeasurementErrorCode_ConnectionToSensor = -100, /**< No connection to sensor */
38 MeasurementErrorCode_DeviceID = -101, /**< Invalid device ID */
39 MeasurementErrorCode_Pointer = -102, /**< Invalid pointer */
40 MeasurementErrorCode_Unknown = -103, /**< Unknown error */
41 MeasurementErrorCode_InvalidDataSize = -104, /**< Invalid data size */
42 MeasurementErrorCode_DataArrayFormat = -151, /**< Invalid data array format */
43 MeasurementErrorCode_NoParameterSet = -161, /**< No parameter set present */
44 MeasurementErrorCode_SetParameter = -162, /**< Error on setting the parameters */
45 MeasurementErrorCode_ReadCameraImg = -163, /**< Error on reading a camera image */
46 MeasurementErrorCode_WriteParameter = -164, /**< Error on writing a parameter */
47 MeasurementErrorCode_ReadParameter = -165, /**< Error on reading a parameter */
48 MeasurementErrorCode_ReadParameterLimits = -166, /**< Error on reading parameter limits */
49 MeasurementErrorCode_ParameterNotAvailable = -167, /**< Parameter not available for this functionality */
50 MeasurementErrorCode_ParameterOutsideOfLimits = -168, /**< Parameter outside of limits */
51 MeasurementErrorCode_ParameterExists = -169, /**< Parameter already exists */
52 MeasurementErrorCode_ParameterNotExists = -170, /**< Parameter not exists */
53 MeasurementErrorCode_InitParameter = -171, /**< Error on initializing a parameter */
54 MeasurementErrorCode_ArrayIndex = -172, /**< Invalid array index */
55 MeasurementErrorCode_DataConversion = -173, /**< Error on data conversion */
56 MeasurementErrorCode_InvalidSensorType = -174, /**< Invalid sensor type */
57 MeasurementErrorCode_InvalidParameterType = -175, /**< Invalid parameter type */
58 MeasurementErrorCode_ReadTextureImg = -176, /**< Error on reading a texture image */
59
60 MeasurementErrorCode_WrongMeasMode = -181, /**< Wrong measurement mode */
61
62 MeasurementErrorCode_MeasParamSet = -201, /**< Invalid measurement parameter set */
63 MeasurementErrorCode_FilterParamSet = -202, /**< Invalid filter parameter set */
64 MeasurementErrorCode_Filter = -203, /**< Error on filter */
65 MeasurementErrorCode_MeasProgNameExists = -204, /**< Measurement program name already exists */
66 MeasurementErrorCode_MeasProgNotExists = -205, /**< Measurement program name not exists */
67
68 MeasurementErrorCode_NoDataTransfer = -300, /**< Error no data transfer available */
69 MeasurementErrorCode_InvalidDataTransferID = -301, /**< Error invalid data transfer ID */
70 MeasurementErrorCode_DataTransfer = -302, /**< Error on data transfer */
71 MeasurementErrorCode_ReadDataFromSensor = -303, /**< Error on reading measurement data from sensor */
72 MeasurementErrorCode_WriteDataToSensor = -304, /**< Error on writing measurement data to sensor */
73
74 // Sequence errors
75
76 MeasurementErrorCode_SequenceTooMuchImages = -1001, /**< Too much images */
77 MeasurementErrorCode_SequenceFormat = -1002, /**< Invalid sequence format */
78 MeasurementErrorCode_SequenceItem = -1003, /**< Invalid sequence item */
79 MeasurementErrorCode_SequenceIndex = -1004, /**< Invalid sequence index */
80 MeasurementErrorCode_SequenceAlloc = -1005, /**< Error on sequence allocation on sensor */
81 MeasurementErrorCode_SequenceImageToSensor = -1006, /**< Error on putting an image to a sequence on sensor */
82 MeasurementErrorCode_SequenceProjectImage = -1007, /**< Error on project a sequence image */
83 MeasurementErrorCode_SequenceStart = -1008, /**< Error on starting a sequence */
84 MeasurementErrorCode_SequenceStop = -1009, /**< Error on stopping a sequence */
85 MeasurementErrorCode_SequenceAdd = -1010, /**< Error on adding a sequence */
86 MeasurementErrorCode_MeasSequenceItem = -1021, /**< Invalid measurement sequence item (Gray code line, phase shift line ...) */
87 MeasurementErrorCode_SequenceTiming = -1022, /**< Error on setting the sequence timing parameters */
88 MeasurementErrorCode_SequenceNoImage = -1023, /**< No image in the sequence */
89 MeasurementErrorCode_SequenceTexture = -1024, /**< Error on loading the texture sequence to the sensor */
90
91 // Buffer error
92
93 MeasurementErrorCode_NumBufferItems = -1101, /**< Invalid number of buffer items */
94
95
96 // Data acquisition
97
98 MeasurementErrorCode_NotEnoughValidData = -1201, /**< Not enough valid data */
99 MeasurementErrorCode_CalcXYZ = -1202, /**< Error on calculating XYZ coordinates */
100 MeasurementErrorCode_OutData = -1203, /**< Error on calculating output data */
101 MeasurementErrorCode_GetCameraImage = -1204, /**< Error on getting a camera image */
102 MeasurementErrorCode_ProjectImage = -1205, /**< Error on projecting a image */
103 MeasurementErrorCode_PreFilter = -1221, /**< Error on pre-filtering */
104
105
106 // Calibration
107
108 MeasurementErrorCode_NotCalib = -1301, /**< System not calibrated */
109 MeasurementErrorCode_CalibData = -1302, /**< Missing or wrong calibration data */
110 MeasurementErrorCode_CalibHeightImg = -1303, /**< Error on height image calibration */
111 MeasurementErrorCode_InvalidCalibMode = -1304, /**< Invalid calibration mode */
112 MeasurementErrorCode_CalibCalcPlane = -1305, /**< Error on calculation of plane calibration */
113 MeasurementErrorCode_CalibCalcGroove = -1306, /**< Error on calculation of groove calibration */
114 MeasurementErrorCode_CalibReadParameter = -1307, /**< Error on reading calibration parameters */
115 MeasurementErrorCode_CalibWriteParameter = -1308, /**< Error on writing calibration parameters */
116 MeasurementErrorCode_CalibAOI = -1309, /**< Calibration AOI different to measurement AOI */
117 MeasurementErrorCode_WrongCalibMode = -1310, /**< Wrong calibration mode */
118 MeasurementErrorCode_CalibPowerSpectrum = -1311, /**< Error on using power spectrum (after calibration) */
119
120 // Evaluation
121
122 MeasurementErrorCode_Calculation = -1401, /**< Error on calculation */
123
124 MeasurementErrorCode_TooLittleValues = -1421, /**< Too little (valid) values */
125
126
127 // Camera / projector
128
129 MeasurementErrorCode_CameraDriver = -1491, /**< Invalid or missing camera driver */
130 MeasurementErrorCode_ProjectorDriver = -1492, /**< Invalid or missing projector driver */
131
132 MeasurementErrorCode_Camera = -1501, /**< General camera error */
133 MeasurementErrorCode_GrabTimeout = -1502, /**< Camera grab timeout */
134 MeasurementErrorCode_InvalidPixelFormat = -1503, /**< Invalid pixel format */
135 MeasurementErrorCode_InvalidFrameNumber = -1504, /**< Invalid camera frame number */
136 MeasurementErrorCode_InvalidFrameSize = -1505, /**< Invalid camera frame size */
137
138 MeasurementErrorCode_Projector = -1541, /**< General projector error */
139
140 MeasurementErrorCode_DeviceNotRegistered = -1581, /**< Device (projector, camera...) not registered */
141 MeasurementErrorCode_DeviceNotFound = -1582, /**< Device with a specific ID (projector, camera...) not found */
142 MeasurementErrorCode_OpenDevice = -1583, /**< Error on opening a device */
143 MeasurementErrorCode_ProjectorCameraSync = -1584, /**< Error on synchronizing projector - camera */
144 MeasurementErrorCode_ListDevices = -1585, /**< Error on listing devices (cameras, projectors ...) */
145
146 // Configuration
147
148 MeasurementErrorCode_ConfigReadMeasProg = -9001, /**< Error on reading measurement program parameters */
149 MeasurementErrorCode_ConfigWriteMeasProg = -9002, /**< Error on writing measurement program parameters */
150 MeasurementErrorCode_ConfigMeasProgTransferToSensor = -9003, /**< Error on transfer of the program parameters to the sensor */
151 MeasurementErrorCode_ConfigMeasProgTransferFromSensor = -9004, /**< Error on transfer of the program parameters from the sensor */
152 MeasurementErrorCode_ConfigReadAdjustments = -9021, /**< Error on reading adjustments */
153 MeasurementErrorCode_ConfigWriteAdjustments = -9022, /**< Error on writing adjustments */
154 MeasurementErrorCode_ConfigAdjustmentsTransferToSensor = -9023, /**< Error on transfer of the adjustments to the sensor */
155 MeasurementErrorCode_ConfigAdjustmentsTransferFromSensor = -9024, /**< Error on transfer of the adjustments from the sensor */
156 MeasurementErrorCode_ConfigReadBasisConfig = -9025, /**< Error on reading the basis configuration */
157 MeasurementErrorCode_ConfigWriteBasisConfig = -9026, /**< Error on writing the basis configuration */
158 MeasurementErrorCode_ConfigReadCalibData = -9027, /**< Error on reading the calibration data */
159 MeasurementErrorCode_ConfigWriteCalibData = -9028, /**< Error on writing the calibration data */
160 MeasurementErrorCode_ConfigReadData = -9029, /**< Error on reading general data */
161 MeasurementErrorCode_ConfigWriteData = -9030, /**< Error on writing general data */
162 MeasurementErrorCode_ConfigWrongSensorType = -9031, /**< Configuration for wrong sensor type */
163 MeasurementErrorCode_ConfigReadHeaderData = -9032, /**< Error on reading the header data */
164 MeasurementErrorCode_ConfigWriteHeaderData = -9033, /**< Error on writing the header data */
165 };
166
167 #endif // _MeasurementErrorCodes_h
MeasurementErrorCode_SequenceStart
Error on starting a sequence.
Definition: MeasurementErrorCodes.h:83
MeasurementErrorCode_FileAlreadyExists
File already exists.
Definition: MeasurementErrorCodes.h:35
MeasurementErrorCode_Initializing
Error on initializing.
Definition: MeasurementErrorCodes.h:21
MeasurementErrorCode_None
No error.
Definition: MeasurementErrorCodes.h:16
MeasurementErrorCode_SequenceAdd
Error on adding a sequence.
Definition: MeasurementErrorCodes.h:85
MeasurementErrorCode_ArrayIndex
Invalid array index.
Definition: MeasurementErrorCodes.h:54
MeasurementErrorCode_SequenceProjectImage
Error on project a sequence image.
Definition: MeasurementErrorCodes.h:82
MeasurementErrorCode_ConfigReadCalibData
Error on reading the calibration data.
Definition: MeasurementErrorCodes.h:158
MeasurementErrorCode_InvalidPixelFormat
Invalid pixel format.
Definition: MeasurementErrorCodes.h:134
MeasurementErrorCode_WriteParameter
Error on writing a parameter.
Definition: MeasurementErrorCodes.h:46
MeasurementErrorCode_DataConversion
Error on data conversion.
Definition: MeasurementErrorCodes.h:55
MeasurementErrorCode_Unknown
Unknown error.
Definition: MeasurementErrorCodes.h:40
MeasurementErrorCode_DeviceNotRegistered
Device (projector, camera...) not registered.
Definition: MeasurementErrorCodes.h:140
MeasurementErrorCode_MeasProgNameExists
Measurement program name already exists.
Definition: MeasurementErrorCodes.h:65
MeasurementErrorCode_CameraDriver
Invalid or missing camera driver.
Definition: MeasurementErrorCodes.h:129
MeasurementErrorCode_CalibWriteParameter
Error on writing calibration parameters.
Definition: MeasurementErrorCodes.h:115
MeasurementErrorCode_InvalidFileFormat
Invalid file format.
Definition: MeasurementErrorCodes.h:24
MeasurementErrorCode_ConfigReadData
Error on reading general data.
Definition: MeasurementErrorCodes.h:160
MeasurementErrorCode_CalibAOI
Calibration AOI different to measurement AOI.
Definition: MeasurementErrorCodes.h:116
MeasurementErrorCode_DataArrayFormat
Invalid data array format.
Definition: MeasurementErrorCodes.h:42
MeasurementErrorCode_MeasSequenceItem
Invalid measurement sequence item (Gray code line, phase shift line ...)
Definition: MeasurementErrorCodes.h:86
MeasurementErrorCode_CalibCalcGroove
Error on calculation of groove calibration.
Definition: MeasurementErrorCodes.h:113
MeasurementErrorCode_FunctionNotImplemented
Function is not implemented.
Definition: MeasurementErrorCodes.h:22
MeasurementErrorCode_Camera
General camera error.
Definition: MeasurementErrorCodes.h:132
MeasurementErrorCode_SequenceItem
Invalid sequence item.
Definition: MeasurementErrorCodes.h:78
MeasurementErrorCode_DeviceID
Invalid device ID.
Definition: MeasurementErrorCodes.h:38
MeasurementErrorCode_SequenceTooMuchImages
Too much images.
Definition: MeasurementErrorCodes.h:76
MeasurementErrorCode_ParameterExists
Parameter already exists.
Definition: MeasurementErrorCodes.h:51
MeasurementErrorCode_CalibPowerSpectrum
Error on using power spectrum (after calibration)
Definition: MeasurementErrorCodes.h:118
MeasurementErrorCode_WrongMeasMode
Wrong measurement mode.
Definition: MeasurementErrorCodes.h:60
MeasurementErrorCode_ConfigReadBasisConfig
Error on reading the basis configuration.
Definition: MeasurementErrorCodes.h:156
MeasurementErrorCode_ReadDataFromSensor
Error on reading measurement data from sensor.
Definition: MeasurementErrorCodes.h:71
MeasurementErrorCode_CalibData
Missing or wrong calibration data.
Definition: MeasurementErrorCodes.h:109
MeasurementErrorCode_TooLittleValues
Too little (valid) values.
Definition: MeasurementErrorCodes.h:124
MeasurementErrorCode_ConnectionToSensor
No connection to sensor.
Definition: MeasurementErrorCodes.h:37
MeasurementErrorCode_SequenceAlloc
Error on sequence allocation on sensor.
Definition: MeasurementErrorCodes.h:80
MeasurementErrorCode_ConfigWriteBasisConfig
Error on writing the basis configuration.
Definition: MeasurementErrorCodes.h:157
MeasurementErrorCode_InvalidSensorType
Invalid sensor type.
Definition: MeasurementErrorCodes.h:56
MeasurementErrorCode_InvalidCalibMode
Invalid calibration mode.
Definition: MeasurementErrorCodes.h:111
MeasurementErrorCode_GetCameraImage
Error on getting a camera image.
Definition: MeasurementErrorCodes.h:101
MeasurementErrorCode_SequenceTexture
Error on loading the texture sequence to the sensor.
Definition: MeasurementErrorCodes.h:89
MeasurementErrorCode_ProjectorCameraSync
Error on synchronizing projector - camera.
Definition: MeasurementErrorCodes.h:143
MeasurementErrorCode_CalibCalcPlane
Error on calculation of plane calibration.
Definition: MeasurementErrorCodes.h:112
MeasurementErrorCode_InvalidDataTransferID
Error invalid data transfer ID.
Definition: MeasurementErrorCodes.h:69
MeasurementErrorCode_SensorLibraryFunc
Error on loading sensor library function.
Definition: MeasurementErrorCodes.h:28
MeasurementErrorCode_NotEnoughValidData
Not enough valid data.
Definition: MeasurementErrorCodes.h:98
MeasurementErrorCode_WriteDataToSensor
Error on writing measurement data to sensor.
Definition: MeasurementErrorCodes.h:72
MeasurementErrorCode_GrabTimeout
Camera grab timeout.
Definition: MeasurementErrorCodes.h:133
MeasurementErrorCode_ConfigWriteMeasProg
Error on writing measurement program parameters.
Definition: MeasurementErrorCodes.h:149
MeasurementErrorCode_InvalidDataSize
Invalid data size.
Definition: MeasurementErrorCodes.h:41
MeasurementErrorCode_ListDevices
Error on listing devices (cameras, projectors ...)
Definition: MeasurementErrorCodes.h:144
MeasurementErrorCode_Pointer
Invalid pointer.
Definition: MeasurementErrorCodes.h:39
MeasurementErrorCode_ParameterNotExists
Parameter not exists.
Definition: MeasurementErrorCodes.h:52
MeasurementErrorCode_ReadCameraImg
Error on reading a camera image.
Definition: MeasurementErrorCodes.h:45
MeasurementErrorCode_ConfigReadAdjustments
Error on reading adjustments.
Definition: MeasurementErrorCodes.h:152
MeasurementErrorCode_CalibReadParameter
Error on reading calibration parameters.
Definition: MeasurementErrorCodes.h:114
MeasurementErrorCode_WrongCalibMode
Wrong calibration mode.
Definition: MeasurementErrorCodes.h:117
MeasurementErrorCode_SequenceFormat
Invalid sequence format.
Definition: MeasurementErrorCodes.h:77
MeasurementErrorCode_BufferLocked
A buffer is locked.
Definition: MeasurementErrorCodes.h:30
MeasurementErrorCode_SequenceNoImage
No image in the sequence.
Definition: MeasurementErrorCodes.h:88
MeasurementErrorCode_ConfigReadHeaderData
Error on reading the header data.
Definition: MeasurementErrorCodes.h:163
MeasurementErrorCode_DirectoryNotExists
Directory not exists.
Definition: MeasurementErrorCodes.h:33
MeasurementErrorCode_ReadParameterLimits
Error on reading parameter limits.
Definition: MeasurementErrorCodes.h:48
MeasurementErrorCode_ConfigWriteAdjustments
Error on writing adjustments.
Definition: MeasurementErrorCodes.h:153
MeasurementErrorCode_Calculation
Error on calculation.
Definition: MeasurementErrorCodes.h:122
MeasurementErrorCode_InvalidParameterType
Invalid parameter type.
Definition: MeasurementErrorCodes.h:57
MeasurementErrorCode_CheckSumError
Check sum error.
Definition: MeasurementErrorCodes.h:31
MeasurementErrorCode_InvalidFrameSize
Invalid camera frame size.
Definition: MeasurementErrorCodes.h:136
MeasurementErrorCode_ParameterNotAvailable
Parameter not available for this functionality.
Definition: MeasurementErrorCodes.h:49
MeasurementErrorCode_ParameterOutsideOfLimits
Parameter outside of limits.
Definition: MeasurementErrorCodes.h:50
MeasurementErrorCode_InvalidFrameNumber
Invalid camera frame number.
Definition: MeasurementErrorCodes.h:135
MeasurementErrorCode_NotCalib
System not calibrated.
Definition: MeasurementErrorCodes.h:108
MeasurementErrorCode_FileSaveError
Cannot save file.
Definition: MeasurementErrorCodes.h:25
MeasurementErrorCode_InitParameter
Error on initializing a parameter.
Definition: MeasurementErrorCodes.h:53
MeasurementErrorCode_SequenceIndex
Invalid sequence index.
Definition: MeasurementErrorCodes.h:79
MeasurementErrorCode
MeasurementErrorCode
Error codes.
Definition: MeasurementErrorCodes.h:14
MeasurementErrorCode_DataTransfer
Error on data transfer.
Definition: MeasurementErrorCodes.h:70
MeasurementErrorCode_ConfigAdjustmentsTransferToSensor
Error on transfer of the adjustments to the sensor.
Definition: MeasurementErrorCodes.h:154
MeasurementErrorCode_PreFilter
Error on pre-filtering.
Definition: MeasurementErrorCodes.h:103
MeasurementErrorCode_CalcXYZ
Error on calculating XYZ coordinates.
Definition: MeasurementErrorCodes.h:99
MeasurementErrorCode_ReadParameter
Error on reading a parameter.
Definition: MeasurementErrorCodes.h:47
MeasurementErrorCode_DeviceNotFound
Device with a specific ID (projector, camera...) not found.
Definition: MeasurementErrorCodes.h:141
MeasurementErrorCode_ConfigMeasProgTransferToSensor
Error on transfer of the program parameters to the sensor.
Definition: MeasurementErrorCodes.h:150
MeasurementErrorCode_OutData
Error on calculating output data.
Definition: MeasurementErrorCodes.h:100
MeasurementErrorCode_NumBufferItems
Invalid number of buffer items.
Definition: MeasurementErrorCodes.h:93
MeasurementErrorCode_SetParameter
Error on setting the parameters.
Definition: MeasurementErrorCodes.h:44
MeasurementErrorCode_MeasProgNotExists
Measurement program name not exists.
Definition: MeasurementErrorCodes.h:66
MeasurementErrorCode_NotInitialized
Not or incorrect initialized.
Definition: MeasurementErrorCodes.h:20
MeasurementErrorCode_ReadTextureImg
Error on reading a texture image.
Definition: MeasurementErrorCodes.h:58
MeasurementErrorCode_ConfigWriteCalibData
Error on writing the calibration data.
Definition: MeasurementErrorCodes.h:159
MeasurementErrorCode_FileNotExists
File not exists.
Definition: MeasurementErrorCodes.h:34
MeasurementErrorCode_ConfigWrongSensorType
Configuration for wrong sensor type.
Definition: MeasurementErrorCodes.h:162
MeasurementErrorCode_ProjectorDriver
Invalid or missing projector driver.
Definition: MeasurementErrorCodes.h:130
MeasurementErrorCode_SensorLibrary
Error on loading sensor library.
Definition: MeasurementErrorCodes.h:27
MeasurementErrorCode_OpenDevice
Error on opening a device.
Definition: MeasurementErrorCodes.h:142
MeasurementErrorCode_ConfigMeasProgTransferFromSensor
Error on transfer of the program parameters from the sensor.
Definition: MeasurementErrorCodes.h:151
MeasurementErrorCode_NoParameterSet
No parameter set present.
Definition: MeasurementErrorCodes.h:43
MeasurementErrorCode_InvalidVersion
Invalid version of a software component.
Definition: MeasurementErrorCodes.h:23
MeasurementErrorCode_SequenceStop
Error on stopping a sequence.
Definition: MeasurementErrorCodes.h:84
MeasurementErrorCode_MeasParamSet
Invalid measurement parameter set.
Definition: MeasurementErrorCodes.h:62
MeasurementErrorCode_CalibHeightImg
Error on height image calibration.
Definition: MeasurementErrorCodes.h:110
MeasurementErrorCode_NoDataTransfer
Error no data transfer available.
Definition: MeasurementErrorCodes.h:68
MeasurementErrorCode_ConfigWriteHeaderData
Error on writing the header data.
Definition: MeasurementErrorCodes.h:164
MeasurementErrorCode_Projector
General projector error.
Definition: MeasurementErrorCodes.h:138
MeasurementErrorCode_SequenceImageToSensor
Error on putting an image to a sequence on sensor.
Definition: MeasurementErrorCodes.h:81
MeasurementErrorCode_ConfigWriteData
Error on writing general data.
Definition: MeasurementErrorCodes.h:161
MeasurementErrorCode_Filter
Error on filter.
Definition: MeasurementErrorCodes.h:64
MeasurementErrorCode_ProjectImage
Error on projecting a image.
Definition: MeasurementErrorCodes.h:102
MeasurementErrorCode_SequenceTiming
Error on setting the sequence timing parameters.
Definition: MeasurementErrorCodes.h:87
MeasurementErrorCode_FilterParamSet
Invalid filter parameter set.
Definition: MeasurementErrorCodes.h:63
MeasurementErrorCode_ConfigReadMeasProg
Error on reading measurement program parameters.
Definition: MeasurementErrorCodes.h:148
MeasurementErrorCode_ConfigAdjustmentsTransferFromSensor
Error on transfer of the adjustments from the sensor.
Definition: MeasurementErrorCodes.h:155