Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_EnableExternalInputZPulse | ( | GoSetup | setup,
|  | kBool | enable
| ) |  |

Sets the state of the external input triggered encoder Z-pulse feature.

Version
  Introduced in firmware 4.1.3.106

Parameters

  setup | GoSetup object.
  enable | kTRUE to enable it and kFALSE to disable it.

Returns
  Operation status.