Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoPartDetection_SetThresholdDirection | ( | GoPartDetection | detection,
|  | GoPartHeightThresholdDirection | direction
| ) |  |

Sets the part detection height threshold direction.

Version
  Introduced in firmware 4.0.10.27

Parameters

  detection | GoPartDetection object.
  direction | The part detection height threshold direction value to set.

Returns
  Operation status.