Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoReplayAnyData_SetRangeCountThreshold | ( | GoReplayAnyData | condition,
|  | k32u | threshold
| ) |  |

Sets the required range count threshold.

Version
  Introduced in firmware 4.5.3.57

Parameters

  condition | GoReplayAnyData object.
  threshold | The required range count threshold.

Returns
  Operation status.