Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_ScheduledStart | ( | GoSensor | sensor,
|  | k64s | value
| ) |  |

Starts the sensor at a scheduled value.

Version
  Introduced in firmware 4.1.3.106

Parameters

  sensor | GoSensor object.
  value | Scheduled start value. uS when time triggered and ticks when encoder triggered.

Returns
  Operation status.

See also
  GoSetup_SetTriggerSource, GoSetup_TriggerSource, GoSystem_Timestamp, GoSystem_Encoder