Gocator API > Go2 > Classes > Go2System > Functions > Go2System_CalibratedX

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_CalibratedX
Functions
Description

Gets the system's active area x-origin, in system coordinates (post-calibration).

C

    Go2Double Go2System_CalibratedX(Go2System system);

Parameters

Parameters | Description
Go2System system | Go2System object.

Returns

System active area x origin, in system coordinates (mm).

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference