Gocator API > Go2.Part > Classes > Go2PartBoundingBoxX > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2PartBoundingBoxX

Go2PartBoundingBoxX Functions

Functions

Function | Description
Go2PartBoundingBoxX_DecisionMax | Gets the decision threshold maximum value.
Go2PartBoundingBoxX_DecisionMin | Gets the decision threshold minimum value.
Go2PartBoundingBoxX_EnableHold | Enables measurement value hold.
Go2PartBoundingBoxX_EnableRotation | Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.
Go2PartBoundingBoxX_EnableSmoothing | Enables measurement value smoothing.
Go2PartBoundingBoxX_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartBoundingBoxX_Id | Gets the unique measurement identifier for the measurement.
Go2PartBoundingBoxX_Name | Gets the descriptive name for the measurement.
Go2PartBoundingBoxX_RotationEnabled | Reports whether bounding box rotation is enabled.
Go2PartBoundingBoxX_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartBoundingBoxX_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartBoundingBoxX_SetId | Sets the unique measurement identifier for the measurement.
Go2PartBoundingBoxX_SetName | Sets the descriptive name for the measurement.
Go2PartBoundingBoxX_SetSmoothingWindow | Sets the smoothing window value.
Go2PartBoundingBoxX_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartBoundingBoxX_SmoothingWindow | Gets the smoothing window value.
Go2PartBoundingBoxX_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartBoundingBoxX_SmoothingWindowMin | Gets the minimum smoothing window value.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference