Gocator API > Go2.Profile > Classes > Go2ProfileHeight > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileHeight_AbsoluteResult | Gets whether this measurement should calculate absolute measurements.
Go2ProfileHeight_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileHeight_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileHeight_EnableHold | Enables measurement value hold.
Go2ProfileHeight_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileHeight_FeatureAt | Gets the feature point at the specified index.
Go2ProfileHeight_FeatureCount | Gets the count of feature points.
Go2ProfileHeight_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileHeight_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileHeight_Name | Gets the descriptive name for the measurement.
Go2ProfileHeight_SetAbsoluteResult | Sets whether this measurement should calculate absolute measurements.
Go2ProfileHeight_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileHeight_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileHeight_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileHeight_SetName | Sets the descriptive name for the measurement.
Go2ProfileHeight_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileHeight_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileHeight_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileHeight_SmoothingWindow | Gets the smoothing window value.
Go2ProfileHeight_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileHeight_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileHeight_Source | Gets the source for profile data used in this measurement.
Go2ProfileHeight_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileHeight_SourceOptionCount | Gets the number of profile source options for the measurement.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference