Gocator API > Go2.Part > Classes > Go2PartBoundingBoxY > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2PartBoundingBoxY

Go2PartBoundingBoxY Functions

Functions

Function | Description
Go2PartBoundingBoxY_DecisionMax | Gets the decision threshold maximum value.
Go2PartBoundingBoxY_DecisionMin | Gets the decision threshold minimum value.
Go2PartBoundingBoxY_EnableHold | Enables measurement value hold.
Go2PartBoundingBoxY_EnableRotation | Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.
Go2PartBoundingBoxY_EnableSmoothing | Enables measurement value smoothing.
Go2PartBoundingBoxY_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartBoundingBoxY_Id | Gets the unique measurement identifier for the measurement.
Go2PartBoundingBoxY_Name | Gets the descriptive name for the measurement.
Go2PartBoundingBoxY_RotationEnabled | Reports whether bounding box rotation is enabled.
Go2PartBoundingBoxY_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartBoundingBoxY_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartBoundingBoxY_SetId | Sets the unique measurement identifier for the measurement.
Go2PartBoundingBoxY_SetName | Sets the descriptive name for the measurement.
Go2PartBoundingBoxY_SetSmoothingWindow | Sets the smoothing window value.
Go2PartBoundingBoxY_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartBoundingBoxY_SmoothingWindow | Gets the smoothing window value.
Go2PartBoundingBoxY_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartBoundingBoxY_SmoothingWindowMin | Gets the minimum smoothing window value.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference