Gocator API > Go2.Profile > Classes > Go2ProfileBridgeValue > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileBridgeValue_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileBridgeValue_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileBridgeValue_EnableHold | Enables measurement value hold.
Go2ProfileBridgeValue_EnableNormalize | Enables tilt normalization.
Go2ProfileBridgeValue_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileBridgeValue_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileBridgeValue_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileBridgeValue_MaxInvalid | Gets the percentage of profile points which can be invalid before the measurement is invalid.
Go2ProfileBridgeValue_Name | Gets the descriptive name for the measurement.
Go2ProfileBridgeValue_NormalizeEnabled | Determines if tilt normalization is enabled.
Go2ProfileBridgeValue_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileBridgeValue_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileBridgeValue_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileBridgeValue_SetMaxInvalid | Sets the percentage of profile points which can be invalid before the measurement is invalid.
Go2ProfileBridgeValue_SetName | Sets the descriptive name for the measurement.
Go2ProfileBridgeValue_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileBridgeValue_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileBridgeValue_SetWindowSize | Sets the percentage of profile points in the window.
Go2ProfileBridgeValue_SetWindowSkip | Sets the percentage of profile points to skip to find the starting point in the window.
Go2ProfileBridgeValue_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileBridgeValue_SmoothingWindow | Gets the smoothing window value.
Go2ProfileBridgeValue_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileBridgeValue_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileBridgeValue_Source | Gets the source for profile data used in this measurement.
Go2ProfileBridgeValue_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileBridgeValue_SourceOptionCount | Gets the number of profile source options for the measurement.
Go2ProfileBridgeValue_WindowSize | Gets the percentage of profile points in the window.
Go2ProfileBridgeValue_WindowSkip | Gets the percentage of profile points to skip to find the starting point in the window.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference