Gocator API > Go2.Profile > Classes > Go2ProfileWidth > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileWidth_AbsoluteResult | Gets whether this measurement should calculate absolute measurements.
Go2ProfileWidth_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileWidth_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileWidth_EnableHold | Enables measurement value hold.
Go2ProfileWidth_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileWidth_FeatureAt | Gets the feature point at the specified index.
Go2ProfileWidth_FeatureCount | Gets the count of feature points.
Go2ProfileWidth_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileWidth_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileWidth_Name | Gets the descriptive name for the measurement.
Go2ProfileWidth_SetAbsoluteResult | Sets whether this measurement should calculate absolute measurements.
Go2ProfileWidth_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileWidth_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileWidth_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileWidth_SetName | Sets the descriptive name for the measurement.
Go2ProfileWidth_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileWidth_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileWidth_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileWidth_SmoothingWindow | Gets the smoothing window value.
Go2ProfileWidth_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileWidth_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileWidth_Source | Gets the source for profile data used in this measurement.
Go2ProfileWidth_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileWidth_SourceOptionCount | Gets the number of profile source options for the measurement.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference