Gocator API > Go2.Profile > Classes > Go2ProfileAngleX > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2ProfileAngleX

Go2ProfileAngleX functions.

Functions

Function | Description
Go2ProfileAngleX_AbsoluteResult | Gets whether this measurement should calculate absolute measurements.
Go2ProfileAngleX_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileAngleX_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileAngleX_EnableHold | Enables measurement value hold.
Go2ProfileAngleX_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileAngleX_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileAngleX_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileAngleX_Line | Gets the fit line object.
Go2ProfileAngleX_Name | Gets the descriptive name for the measurement.
Go2ProfileAngleX_SetAbsoluteResult | Sets whether this measurement should calculate absolute measurements.
Go2ProfileAngleX_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileAngleX_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileAngleX_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileAngleX_SetName | Sets the descriptive name for the measurement.
Go2ProfileAngleX_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileAngleX_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileAngleX_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileAngleX_SmoothingWindow | Gets the smoothing window value.
Go2ProfileAngleX_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileAngleX_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileAngleX_Source | Gets the source for profile data used in this measurement.
Go2ProfileAngleX_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileAngleX_SourceOptionCount | Gets the number of profile source options for the measurement.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference