Zen API | Contents | Reference | Previous | Up | Next

zFireSync_SetAddress
zFireSync functions
C

    zStatus zFireSync_SetAddress(z32u deviceId, const zAddressInfo* address);

Parameters

Parameters | Description
z32u deviceId | Serial number of the server.
const zAddressInfo* address | New address configuration for the server.

Description

Locates a FireSync server by id (serial number) and configures its network address settings.

Remarks

This function uses UDP broadcast messages to locate FHP servers. The servers and client may be on different subnets.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference