Gocator API > Go2.Output > Classes > Go2Digital > Functions

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2Digital

Go2Digital functions.

Functions

Function | Description
Go2Digital_AddSource | Selects the specified decision source for use in determining pass/fail status.
Go2Digital_ClearSources | Removes all selected decision sources.
Go2Digital_Delay | Gets the output delay.
Go2Digital_EnableSchedule | Enables or disables the scheduler for this output
Go2Digital_Event | Gets the event which triggers this output to fire
Go2Digital_Id | Gets the id of this output.
Go2Digital_OptionAt | Gets the decision source option at the specified index.
Go2Digital_OptionCount | Gets the number of available decision source options.
Go2Digital_PassMode | Gets the pass/fail mode for the digital output.
Go2Digital_PulseWidth | Gets the width of digital output pulses.
Go2Digital_PulseWidthLimitMax | Gets the maximum valid value for the PulseWidth setting.
Go2Digital_PulseWidthLimitMin | Gets the minimum valid value for the PulseWidth setting.
Go2Digital_RemoveSource | Removes (deselects) the decision source at the specified index.
Go2Digital_ScheduleEnabled | Gets the enabled state of the scheduler for this output
Go2Digital_SetDelay | Sets the delay from exposure until output is triggered, in units based on SyncDomain. mm when SyncDomain is distance, us when SyncDomain is time. Ignored when SyncDomain is Immediate or when PassMode is Software
Go2Digital_SetEvent | Sets the event which triggers this output to fire
Go2Digital_SetPassMode | Sets the pass/fail mode for the digital output.
Go2Digital_SetPulseWidth | Sets the width of digital output pulses.
Go2Digital_SetSignalType | Sets the signal type of output.
Go2Digital_SignalType | Gets the signal type of output.
Go2Digital_SourceAt | Gets the identifier of the selected output source at the specified index.
Go2Digital_SourceCount | Gets the number of decision sources that are currently selected for determining pass/fail state.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference