Zen API | Contents | Reference | Previous | Up | Next

zFireSync_GetAddress
zFireSync functions
C

    zStatus zFireSync_GetAddress(z32u deviceId, zAddressInfo* address);

Parameters

Parameters | Description
z32u deviceId | Serial number of the server.
zAddressInfo* address | Receives current address configuration if the server was found.

Description

Locates a FireSync server by id (serial number) and reports its network address settings.

Remarks

This function uses UDP broadcast messages to locate FHP servers. The servers and client may be on different subnets.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference