Zen API | Contents | Reference | Previous | Up | Next

zFireSync_BeginUpgrade
zFireSync functions
C

    zStatus zFireSync_BeginUpgrade(zFireSync fireSync, const zByte* data, zUIntPtr size);

Parameters

Parameters | Description
zFireSync fireSync | zFireSync object.
const zByte* data | Contents of the upgrade package file (provided by LMI Technologies).
zUIntPtr size | Size of the upgrade package file, in bytes.

Description

Initiates a firmware upgrade for devices in the FireSync network.

Remarks

This function uses the Upgrade channel. This function does not wait for the upgrade process to complete - use the zFireSync_GetUpgradeStatus function to determine the current state of the uprade process.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference