Gocator API > Go2.Part > Classes > Go2PartBoundingBoxY > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2PartBoundingBoxY_DecisionMax | Gets the decision threshold maximum value.
Go2PartBoundingBoxY_DecisionMin | Gets the decision threshold minimum value.
Go2PartBoundingBoxY_EnableHold | Enables measurement value hold.
Go2PartBoundingBoxY_EnableLink | Enables or disables measurement linking.
Go2PartBoundingBoxY_EnableRegion | Enables or disables the optional region.
Go2PartBoundingBoxY_EnableRotation | Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.
Go2PartBoundingBoxY_EnableSmoothing | Enables measurement value smoothing.
Go2PartBoundingBoxY_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartBoundingBoxY_Id | Gets the unique measurement identifier for the measurement.
Go2PartBoundingBoxY_Link | Gets the measurement id of the linked measurement.
Go2PartBoundingBoxY_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2PartBoundingBoxY_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartBoundingBoxY_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartBoundingBoxY_Name | Gets the descriptive name for the measurement.
Go2PartBoundingBoxY_Offset | Gets the measurement value offset.
Go2PartBoundingBoxY_Region | Returns the region.
Go2PartBoundingBoxY_RegionEnabled | Returns the current state of the optional region.
Go2PartBoundingBoxY_RotationEnabled | Reports whether bounding box rotation is enabled.
Go2PartBoundingBoxY_Scale | Gets the measurement value scale factor.
Go2PartBoundingBoxY_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartBoundingBoxY_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartBoundingBoxY_SetId | Sets the unique measurement identifier for the measurement.
Go2PartBoundingBoxY_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2PartBoundingBoxY_SetName | Sets the descriptive name for the measurement.
Go2PartBoundingBoxY_SetOffset | Sets the measurement value offset.
Go2PartBoundingBoxY_SetScale | Sets the measurement value scale factor.
Go2PartBoundingBoxY_SetSmoothingWindow | Sets the smoothing window value.
Go2PartBoundingBoxY_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartBoundingBoxY_SmoothingWindow | Gets the smoothing window value.
Go2PartBoundingBoxY_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartBoundingBoxY_SmoothingWindowMin | Gets the minimum smoothing window value.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference