Gocator API > Go2 > Classes > Go2System > Functions > Go2System_IsAuthenticated

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_IsAuthenticated
Functions
Description

Determines if the sensor is in an authenticated state. There can only be a single authenticated connection to the system at a time. This does not return the authentication state of this connection.

C

    Go2Bool Go2System_IsAuthenticated(Go2System system);

Parameters

Parameters | Description
Go2System system | Go2System object.

Returns

GO2_TRUE if the sensor is logged in; GO2_FALSE otherwise.

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference