Gocator API > Go2 > Classes > Go2System > Functions > Go2System_Reconnect

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_Reconnect
Functions
Description

Waits to connect with a sensor that might currently be powering up or resetting.

C

    Go2Status Go2System_Reconnect(Go2System system, Go2IPAddress address);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2IPAddress address | Sensor IP address.

Returns

Certain commands, such Upgrade or Reset, cause the connected sensor to begin an auto-reset sequence. This function can be used to wait a reasonable amount of time to re-establish a connection to a sensor that is currently initializing.

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference