Gocator API > Go2.Part > Classes > Go2PartBoundingBoxLength > Functions > Go2PartBoundingBoxLength_EnableRotation

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2PartBoundingBoxLength_EnableRotation
Functions
Description

Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.

C

    Go2Status Go2PartBoundingBoxLength_EnableRotation(Go2PartBoundingBoxLength measurement, Go2Bool enable);

Parameters

Parameters | Description
Go2PartBoundingBoxLength measurement | Go2PartBoundingBoxLength object.
Go2Bool enable | GO2_TRUE to enable, or GO2_FALSE to disable.

Returns

Operation status.

File

Go2PartBoundingBoxLength.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference