Gocator API > Go2.Output > Values > Go2AnalogEvent

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2AnalogEvent
Values
Description

Represents the event which triggers this output.

C

    enum Go2AnalogEvent {
      GO2_ANALOG_CONTROL_EVENT_MEASURMENT = 1,
      GO2_ANALOG_CONTROL_EVENT_SOFTWARE = 2
    };

Members

Members | Description
GO2_ANALOG_CONTROL_EVENT_MEASURMENT = 1 | Output is measurement driven.
GO2_ANALOG_CONTROL_EVENT_SOFTWARE = 2 | Output is software driven.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference