Gocator API > Go2 > Values > Go2StateIndex

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2StateIndex
Values
Description

Represents the index values for states contained within the array returned by Go2System_GetStates.

C

    enum Go2StateIndex {
      GO2_STATE_INDEX_SYSTEM = 0,
      GO2_STATE_INDEX_CALIBRATION = 1,
      GO2_STATE_INDEX_RECORDING = 2,
      GO2_STATE_INDEX_DATA_SOURCE = 3
    };

Members

Members | Description
GO2_STATE_INDEX_SYSTEM = 0 | System state. Please refer to Go2SystemState for the represented values.
GO2_STATE_INDEX_CALIBRATION = 1 | Calibration state. Please refer to Go2CalibrationState to decode the values.
GO2_STATE_INDEX_RECORDING = 2 | Recording state. It will have a value of 0 if disabled and 1 if enabled.
GO2_STATE_INDEX_DATA_SOURCE = 3 | Playback data source. It will have a value of 0 if the data is live and 1 if the data is from a recording.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference