Gocator API > Go2.Part > Classes > Go2PartEllipseAngle > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2PartEllipseAngle

Go2PartEllipseAngle Functions

Functions

Function | Description
Go2PartEllipseAngle_DecisionMax | Gets the decision threshold maximum value.
Go2PartEllipseAngle_DecisionMin | Gets the decision threshold minimum value.
Go2PartEllipseAngle_EnableHold | Enables measurement value hold.
Go2PartEllipseAngle_EnableLink | Enables or disables measurement linking.
Go2PartEllipseAngle_EnableRegion | Enables or disables the optional region.
Go2PartEllipseAngle_EnableSmoothing | Enables measurement value smoothing.
Go2PartEllipseAngle_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartEllipseAngle_Id | Gets the unique measurement identifier for the measurement.
Go2PartEllipseAngle_Link | Gets the measurement id of the linked measurement.
Go2PartEllipseAngle_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2PartEllipseAngle_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartEllipseAngle_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartEllipseAngle_Name | Gets the descriptive name for the measurement.
Go2PartEllipseAngle_Offset | Gets the measurement value offset.
Go2PartEllipseAngle_Region | Returns the region.
Go2PartEllipseAngle_RegionEnabled | Returns the current state of the optional region.
Go2PartEllipseAngle_Scale | Gets the measurement value scale factor.
Go2PartEllipseAngle_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartEllipseAngle_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartEllipseAngle_SetId | Sets the unique measurement identifier for the measurement.
Go2PartEllipseAngle_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2PartEllipseAngle_SetName | Sets the descriptive name for the measurement.
Go2PartEllipseAngle_SetOffset | Sets the measurement value offset.
Go2PartEllipseAngle_SetScale | Sets the measurement value scale factor.
Go2PartEllipseAngle_SetSmoothingWindow | Sets the smoothing window value.
Go2PartEllipseAngle_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartEllipseAngle_SmoothingWindow | Gets the smoothing window value.
Go2PartEllipseAngle_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartEllipseAngle_SmoothingWindowMin | Gets the minimum smoothing window value.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference