Gocator API > Go2.Part > Classes > Go2PartHoleX > Functions > Go2PartHoleX_SetDecisionMax

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2PartHoleX_SetDecisionMax
Functions
Description

Sets the decision threshold maximum value.

C

    Go2Status Go2PartHoleX_SetDecisionMax(Go2PartHoleX measurement, Go2Double max);

Parameters

Parameters | Description
Go2PartHoleX measurement | Go2PartHoleX object.
Go2Double max | Decision threshold maximum value.

Returns

Operation status.

Remarks

A decision is said to pass if the measurement value is between the minimum and maximum thresholds.

File

Go2PartHoleX.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference