Gocator API > Go2 > Classes > Go2System > Functions > Go2System_CopyFile

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_CopyFile
Functions
Description

Copies a file within the connected sensor.

C

    Go2Status Go2System_CopyFile(Go2System system, const Go2Char* sourceName, const Go2Char* destName);

Parameters

Parameters | Description
Go2System system | Go2System object.
const Go2Char* sourceName | Source name for the file to be copied.
const Go2Char* destName | Destination name for the file (maximum 63 characters).

Returns

Operation status.

Remarks

If the live configuration, transformation, or profile template is specified as the destination name, any pre-existing Go2Sensor handles may be invalidated. Thus, any handles MUST be updated by assigning them with an appropriate Go2System Sensor function.

Calling this function will result in writing operations to flash storage. Should the process be disrupted due to power loss or other factors, the sensor may enter Rescue mode.

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference