Gocator API > Go2.Part > Classes > Go2PartOpeningWidth > Functions > Go2PartOpeningWidth_EnableLink

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2PartOpeningWidth_EnableLink
Functions
Description

Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.

C

    Go2Status Go2PartOpeningWidth_EnableLink(Go2PartOpeningWidth measurement, Go2Bool enable);

Parameters

Parameters | Description
Go2PartOpeningWidth measurement | Go2PartOpeningWidth object.
Go2Bool enable | GO2_TRUE to enable, or GO2_FALSE to disable.

Returns

Operation status.

File

Go2PartOpeningWidth.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference