Gocator API > Go2.Part > Values > Go2PartHeightType

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2PartHeightType
Values
Description

Represents a part height type.

C

    enum Go2PartHeightType {
      GO2_PART_HEIGHT_TYPE_MINIMUM = 0,
      GO2_PART_HEIGHT_TYPE_MAXIMUM = 1,
      GO2_PART_HEIGHT_TYPE_CENTROID_2D = 2,
      GO2_PART_HEIGHT_TYPE_CENTROID_3D = 3,
      GO2_PART_HEIGHT_TYPE_AVERAGE = 4,
      GO2_PART_HEIGHT_TYPE_MEDIAN = 5
    };

Members

Members | Description
GO2_PART_HEIGHT_TYPE_MINIMUM = 0 | Find the minimum height for a part
GO2_PART_HEIGHT_TYPE_MAXIMUM = 1 | Find the maximum height for a part
GO2_PART_HEIGHT_TYPE_CENTROID_2D = 2 | Find the height for a part at the centroid
GO2_PART_HEIGHT_TYPE_CENTROID_3D = 3 | Find the height for a part at the centroid
GO2_PART_HEIGHT_TYPE_AVERAGE = 4 | Find the height for a part based on an average of all the points in the part.
GO2_PART_HEIGHT_TYPE_MEDIAN = 5 | Find the height for a part based on the median of all the points in the part.

File

Go2PartTypes.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference