Gocator API > Go2 > Classes > Go2System > Functions > Go2System_Discover

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2System_Discover
Functions
Description

Locates sensors and reports their network address settings.

C

    Go2Status Go2System_Discover(Go2UInt32** deviceIds, Go2AddressInfo** addresses, Go2UInt32* count);

Parameters

Parameters | Description
Go2UInt32** deviceIds | Receives device identifiers of discovered sensors.
Go2AddressInfo** addresses | Receives network address configurations of discovered sensors.
Go2UInt32* count | Receives count of detected sensors.

Returns

Operation status.

Remarks

This function uses UDP broadcast messages to locate Gocator sensors. The sensors and the client may be on different subnets.

Use the Go2Free function to free the arrays created by this function.

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference