Gocator API > Go2.Profile > Classes > Go2ProfileAngleX > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2ProfileAngleX

Go2ProfileAngleX functions.

Functions

Function | Description
Go2ProfileAngleX_AbsoluteResult | Gets whether this measurement should calculate absolute measurements.
Go2ProfileAngleX_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileAngleX_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileAngleX_EnableHold | Enables measurement value hold.
Go2ProfileAngleX_EnableLink | Enables or disables measurement linking.
Go2ProfileAngleX_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileAngleX_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileAngleX_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileAngleX_Line | Gets the fit line object.
Go2ProfileAngleX_Link | Gets the measurement id of the linked measurement.
Go2ProfileAngleX_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2ProfileAngleX_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2ProfileAngleX_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2ProfileAngleX_Name | Gets the descriptive name for the measurement.
Go2ProfileAngleX_Offset | Gets the measurement value offset.
Go2ProfileAngleX_Scale | Gets the measurement value scale factor.
Go2ProfileAngleX_SetAbsoluteResult | Sets whether this measurement should calculate absolute measurements.
Go2ProfileAngleX_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileAngleX_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileAngleX_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileAngleX_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2ProfileAngleX_SetName | Sets the descriptive name for the measurement.
Go2ProfileAngleX_SetOffset | Sets the measurement value offset.
Go2ProfileAngleX_SetScale | Sets the measurement value scale factor.
Go2ProfileAngleX_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileAngleX_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileAngleX_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileAngleX_SmoothingWindow | Gets the smoothing window value.
Go2ProfileAngleX_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileAngleX_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileAngleX_Source | Gets the source for profile data used in this measurement.
Go2ProfileAngleX_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileAngleX_SourceOptionCount | Gets the number of profile source options for the measurement.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference