Gocator API > Go2.Part > Classes > Go2PartBoundingBoxWidth > Functions

Gocator 3x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2PartBoundingBoxWidth_DecisionMax | Gets the decision threshold maximum value.
Go2PartBoundingBoxWidth_DecisionMin | Gets the decision threshold minimum value.
Go2PartBoundingBoxWidth_EnableHold | Enables measurement value hold.
Go2PartBoundingBoxWidth_EnableLink | Enables or disables measurement linking.
Go2PartBoundingBoxWidth_EnableRegion | Enables or disables the optional region.
Go2PartBoundingBoxWidth_EnableRotation | Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.
Go2PartBoundingBoxWidth_EnableSmoothing | Enables measurement value smoothing.
Go2PartBoundingBoxWidth_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartBoundingBoxWidth_Id | Gets the unique measurement identifier for the measurement.
Go2PartBoundingBoxWidth_Link | Gets the measurement id of the linked measurement.
Go2PartBoundingBoxWidth_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2PartBoundingBoxWidth_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartBoundingBoxWidth_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartBoundingBoxWidth_Name | Gets the descriptive name for the measurement.
Go2PartBoundingBoxWidth_Offset | Gets the measurement value offset.
Go2PartBoundingBoxWidth_Region | Returns the region.
Go2PartBoundingBoxWidth_RegionEnabled | Returns the current state of the optional region.
Go2PartBoundingBoxWidth_RotationEnabled | Reports whether bounding box rotation is enabled.
Go2PartBoundingBoxWidth_Scale | Gets the measurement value scale factor.
Go2PartBoundingBoxWidth_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartBoundingBoxWidth_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartBoundingBoxWidth_SetId | Sets the unique measurement identifier for the measurement.
Go2PartBoundingBoxWidth_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2PartBoundingBoxWidth_SetName | Sets the descriptive name for the measurement.
Go2PartBoundingBoxWidth_SetOffset | Sets the measurement value offset.
Go2PartBoundingBoxWidth_SetScale | Sets the measurement value scale factor.
Go2PartBoundingBoxWidth_SetSmoothingWindow | Sets the smoothing window value.
Go2PartBoundingBoxWidth_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartBoundingBoxWidth_SmoothingWindow | Gets the smoothing window value.
Go2PartBoundingBoxWidth_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartBoundingBoxWidth_SmoothingWindowMin | Gets the minimum smoothing window value.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference